Tips for Installing Solo Cabinet

1. Top Installation
2. If the positioning of holes on the top board is slightly off, and the top board cannot be installed, try pulling out the 4 dowels, (circled below in red).



1. If there is still a gap underneath the top board, this can be rectified by applying pressure onto the top board, (we recommend a rubber hammer for this).



B. Door Installation

a. Installing the hinge in proper order is important; we suggest fitting the lower hinge first, and then following the below steps to install the upper hinges.

* Push the hinge so it is as close to the door as possible.
* Fit screw B into the hinge, **do not tighten it**.
* Fit screw A onto the board while it is in the proper position.
* Tighten screw B only after the door closes correctly.



b. Problems may arise when installing the doors:

* Doors are Not Aligned



Loosen screw A first, then adjust screw B. Note that the hole on hinge for screw B is larger, allowing enough room to adjust screw B to the proper position.

* Gap between 2 Doors.

![C:\Documents and Settings\bakkk\Application Data\Tencent\Users\55327674\QQ\WinTemp\RichOle\)04[4L51[K]7)TSX~QR{YXV.jpg]()

Adjust this particular part of hinge, (circled below in red). This will fix any issues with gaps between the doors.

